LESSINGER
RACING MOTORBOAT 30
LUXURY ELECTRIC HYDROFOIL  |  TECHNICAL DEVELOPMENT SHEET
	30 FT / 9.14 M
LENGTH OVERALL
	100% ELECTRIC
PROPULSION
	27–30 KT
TARGET TOP SPEED


A premium electric hydrofoil runabout developed to combine performance, silence, hydrodynamic efficiency and a distinctive brand identity.
TECHNICAL SPECIFICATIONS
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	Type
	Luxury electric hydrofoil runabout

	Length overall (LOA)
	30 ft / 9.14 m

	Target beam
	2.4–2.5 m

	Target capacity
	5–6 passengers

	Target displacement
	1,700–2,000 kg

	Structure
	Carbon-fibre and fibreglass composites

	Hydrofoils
	Carbon composite – retractable architecture planned

	Propulsion
	100% electric



	
	Target motor power
	50–80 kW

	Target battery capacity
	70–85 kWh

	Target foiling cruise speed
	20–22 knots

	Target top speed
	27–30 knots

	Target range
	45–60 nautical miles

	AC charging
	11–22 kW

	DC fast charging
	To be confirmed during final engineering

	Direct emissions underway
	0





ARCHITECTURE & ON-WATER EXPERIENCE
	HYDROFOIL
Reduced wetted area and drag at cruising speed, targeting a low wake and improved efficiency.
	ELECTRIC
Quiet propulsion, instant torque and zero direct emissions while underway.
	PREMIUM
Sports-runabout architecture, composite materials and luxury positioning for Dubai, Monaco, Miami, Ibiza and the French Riviera.


LESSINGER MOTORBOATS  •  DUBAI
TECHNICAL NOTE — Secondary dimensions, displacement, foil geometry, power, battery capacity, speeds, range and charging characteristics are development targets. They must be validated through naval architecture, hydrodynamic/CFD analysis, prototype testing, electrical integration and certification before being presented as contractual or certified performance figures.
  •  Project basis: LESSINGER Racing Foil / Motorboat file
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